{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Крот_ПРО"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Крот_ПРО","index":0,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[[1,1,1,9],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[5,1,5,2],[3,1,3,4],[3,7,3,9],[12,10,12,11],[10,1,10,2],[13,1,14,4],[16,2,16,4],[4,1,4,2]]}
[]
[null,"Калькулятор для підбору конденсаторів/вітків для Крот ПРО"]
[]
[null,"Ввідні дані:",null,null,null,null,null,"Проміжні результати: (тех.дані)"]
[null,"Бажана частота TX1 =",null,15,"кГц",null,null,"Сумма конд.",{"$f":"D8+D9","v":300},"нФ"]
[null,"Бажана частота Тх2 =",null,7,"кГц",null,null,"Діам. Обм.",{"$f":"ROUNDUP((D7*10/PI()),1)","v":208.5},"мм"]
[null,"Довжина  1 вітка =",null,65.5,"См",null,null,"Опір Тх",{"$f":"ROUND(CoilResistance(I6,D11,D18),2)","v":4.87},"Ом"]
[null,"Конденсатор CB8.1 =",null,65,"нФ",null,null,"Q катушки",{"$f":"ROUND(I12/I7,1)","v":33.5}]
[null,"Конденсатор CB8.2 =",null,235,"нФ",null,null,"Q контура",{"$f":"ROUNDUP(QSC(I10,I7,D8,D10),1)","v":23.8}]
[null,"Резистор RB5 =",null,2,"Ом",null,null,"Інд. Тх1",{"$f":"ROUND(1/(POWER(2*PI()*D5,2)*D8)*1000000000,0)","v":1732},"uH"]
[null,"Діаметр проводу  =",null,0.4,"мм",null,null,"Інд.ТХ2",{"$f":"ROUND(1/(POWER(2*PI()*D6,2)*I5)*1000000000,0)","v":1723},"uH"]
[null,null,null,null,null,null,null,"Хар.опір Тх1",{"$f":"ROUND(SQRT(I10/(D8/1000)),2)","v":163.24},"Ом"]
[null,null,null,null,null,null,null,"Хар.опір Тх2",{"$f":"ROUND(SQRT(I11/(I5/1000)),2)","v":75.78},"Ом"]
[null,"В реузльтаті підбору конденсаторів кількість вітків Тх1 повинно співпасти з Тх2"]
[]
[]
[null,null,"Результат :"]
[null,null,"Тх1",{"$f":"ROUND(CalcCoil(I6,D11,I10),0)","v":55},"Вітків"]
[null,null,"Тх2",{"$f":"ROUND(CalcCoil(I6,D11,I11),0)","v":55},"Вітків"]